#define BLYNK\_TEMPLATE\_ID "TMPLgwKssgggsnFXp"

#define BLYNK\_DEVICE\_NAME "Air Quality Monitoring"

#defineBLYNK\_AUTH\_TOKEN "k03gT6nJosdsfsffesrJV\_S5SXEAdgdsdghhgPZvXEwSKDfj"

#define BLYNK\_PRINT Serial

#include <ESP8266WiFi.h>

#include <BlynkSimpleEsp8266.h>

#include <DHT.h>

//#include <Wire.h>

#include <LiquidCrystal\_I2C.h>

LiquidCrystal\_I2C lcd(0x27, 16, 2);

byte degree\_symbol[8] =

{

0b00111,

0b00101,

0b00111,

0b00000,

0b00000,

0b00000,

0b00000,

0b00000

};

char auth[] = BLYNK\_AUTH\_TOKEN;

char ssid[] = ""; // type your wifi name

char pass[] = ""; // type your wifi password

BlynkTimer timer;

int gas = A0;

int sensorThreshold = 100;

#define DHTPIN 2 //Connect Out pin to D2 in NODE MCU

#define DHTTYPE DHT11

DHT dht(DHTPIN, DHTTYPE);

void sendSensor()

{

float h = dht.readHumidity();

float t = dht.readTemperature(); // or dht.readTemperature(true) for Fahrenheit

if (isnan(h) || isnan(t)) {

Serial.println("Failed to read from DHT sensor!");

return;

}

int analogSensor = analogRead(gas);

Blynk.virtualWrite(V2, analogSensor);

Serial.print("Gas Value: ");

Serial.println(analogSensor);

// You can send any value at any time.

// Please don't send more that 10 values per second.

Blynk.virtualWrite(V0, t);

Blynk.virtualWrite(V1, h);

Serial.print("Temperature : ");

Serial.print(t);

Serial.print(" Humidity : ");

Serial.println(h);

}

void setup()

{

Serial.begin(115200);

//pinMode(gas, INPUT);

Blynk.begin(auth, ssid, pass);

dht.begin();

timer.setInterval(30000L, sendSensor);

//Wire.begin();

lcd.begin();

// lcd.backlight();

// lcd.clear();

lcd.setCursor(3,0);

lcd.print("Air Quality");

lcd.setCursor(3,1);

lcd.print("Monitoring");

delay(2000);

lcd.clear();

}

void loop()

{

Blynk.run();

timer.run();

float h = dht.readHumidity();

float t = dht.readTemperature(); // or dht.readTemperature(true) for Fahrenheit

int gasValue = analogRead(gas);

lcd.setCursor(0,0);

lcd.print("Temperature ");

lcd.setCursor(0,1);

lcd.print(t);

lcd.setCursor(6,1);

lcd.write(1);

lcd.createChar(1, degree\_symbol);

lcd.setCursor(7,1);

lcd.print("C");

delay(4000);

lcd.clear();

lcd.setCursor(0, 0);

lcd.print("Humidity ");

lcd.print(h);

lcd.print("%");

delay(4000);

lcd.clear();

//lcd.setCursor(0,0);

// lcd.print(gasValue);

// lcd.clear();

if(gasValue<600)

{

lcd.setCursor(0,0);

lcd.print("Gas Value: ");

lcd.print(gasValue);

lcd.setCursor(0, 1);

lcd.print("Fresh Air");

Serial.println("Fresh Air");

delay(4000);

lcd.clear();

}

else if(gasValue>600)

{

lcd.setCursor(0,0);

lcd.print(gasValue);

lcd.setCursor(0, 1);

lcd.print("Bad Air");

Serial.println("Bad Air");

delay(4000);

lcd.clear();

}

if(gasValue > 600){

//Blynk.email("shameer50@gmail.com", "Alert", "Bad Air!");

Blynk.logEvent("pollution\_alert","Bad Air");

}

}